Compact Hepa Filter 
Manufactured, tested, and certified at Arabo Filter’s advanced cleanroom production facility, the Box Type HEPA Filter is engineered to deliver high-efficiency particle retention with minimal resistance. Compliant with EN-1822 & ISO-29463, our box filters provide superior filtration performance while maintaining stable airflow, making them ideal for precision-controlled environments.
With rigid media construction and European-grade materials, these filters handle airflow up to 2000 CFM (~3,400 m³/hr), capturing particles ≥0.3 µm. The robust design ensures long service life, low energy use, and stable operation in demanding HVAC and cleanroom settings.

· Compliant with EN-1822 & ISO-29463; factory-tested for ≥99.99% efficiency at H14.
· Built with TAPPI-tested European media, pleated and assembled in ISO-class cleanrooms.
· Available in standard and custom sizes: frame depths 150–300 mm, plastic or galvanized steel frames, operating up to 80 °C.
[image: ]


Markets/applications section
Oil & Gas // Petrochemical // Pharmaceutical // Food & Beverage // Water treatment
Related Products:
Cation Tank – Filter Housing–  Hydraulic Filter
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