Oil Separator
[image: ]Arabo Oil Separator Filter uses high-surface pleated media to coalesce oil mist efficiently, safeguarding downstream compressed air systems with minimal pressure loss and extended operational reliability
Arabo Oil Separator Filter features deep-bed pleated borosilicate media that enhances surface area without enlarging the element, delivering oil residue levels as low as 2–3 ppm. Operating initially at ~0.1–0.2 bar pressure drops and rated for temperatures up to ~110 °C and collapse resistance up to 5 bar, this filter ensures superior oil removal and structural stability

Key Features & Advantages
· Deep-pleated borosilicate fiber media increases filtration surface for high capacity.
· Residual oil content down to 2–3 ppm makes it ideal for compressors and vacuum systems.
· Initial pressure drops as low as ~0.1–0.2 bar minimizes energy loss.
· Collapsible-resistant design rated to ~5 bar pressure resistance.
· Tested under high-specification standards (including ATEX-capable for hazardous atmospheres)

Markets / Applications
Ideal for compressed air or vacuum systems in:
· Industrial screw compressors (oil‑lubricated)
· Vacuum pump systems (laboratory, medical, engineering)
· Manufacturing facilities requiring ultra‑clean air
· Petrochemical and oil & gas processing units
· ATEX-rated installations in hazardous environments
Protects against downstream oil carryover, reduces maintenance, and preserves air quality.
RELATED PRODUCTS: Gas Turbine Filter – Filter Bags – Dust Collector Bags 
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