Packing Support Grid
Arabo manufactures multi‑beam packing support grids alongside pall rings, offering a full-package solution tailored to each project. Our products are fully customized and engineered to fit your process requirements precisely.
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Our multi‑beam packing supports are available in stainless steel 304 and 316, engineered to handle tower internals up to 100 °C (or higher per request) with low pressure drop designs. Each beam is precisely sized (typically ≈ 290 mm wide × 250–300 mm high) with openings under 10 mm to avoid packing migration. The design features separated gas and liquid paths to enhance mass‑transfer efficiency, with sectional construction for ease of installation in columns up to 5m+ diameter.

· Materials: SS 304 or SS 316, optionally carbon steel or specialty alloys
· Beam width: ~290 mm, height range 250‑300 mm per module
· Opening pitch: ≤ 10 mm, customizable patterns (slot, round, square)
· Open‑area ratio: up to 100 %, ensuring minimal pressure drop (< 20 Pa)
· Load capacity: high stiffness for deep beds and dynamic liquid hold‑up
· Modular/sectional design suited for man‑way access and installation
· Compatible with ring and saddle type random packing, engineered for distillation, absorption and washing towers
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