Vane type Mist Eliminator
[image: Mist Eliminators | Vane Type & Ultra Mist Eliminators - Finepac]Arabo manufactures high‑performance vane‑type mist eliminators alongside the full suite of distillation tower internals we offer, delivering a complete, engineered solution tailored to each project.
Our mist eliminators are built in 304 or 316 stainless steel, designed to remove droplets in the 10 µm to 40 µm range with exceptionally low pressure drop (< 0.5 m/s gas velocity or higher depending on profile). Typical configurations mirror industry standards—such as pocketed vanes or chevron‑type banks—to achieve 95–99% efficiency while maintaining face velocities up to 0.45 m/s.
· Manufactured with precise vane spacing and drainage hooks to control flow direction and coalescence
· Capacity factors based on Souders‑Brown equation, tailored for vertical or horizontal installations
· Co-built with pall rings for full phase‑separation systems, enabling compact vessel size and consistent performance
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Related Products:
Wire Mesh Mist Eliminator – Pall rings – Bubble Cap 
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