Water Separator
[image: ]Arabo water separator blends six-layer microfiber glass coalescing and activated carbon adsorption within a stainless‑steel, aluminum or polymer housing to eliminate aerosols, moisture, rust, oil and sub‑micron particulates. Delivers dry, odor‑free gas with minimal pressure drop in a compact, in‑line configuration. 
Six-layer glass‑microfiber element rated 1–5 µm achieves ≥ 99.99999 % retention of droplets and particulates. Carbon‑adsorbent stage removes oil vapor and odor. Installed in stainless, aluminum or polymer vessels rated to 16 bars. Integrated gravity or float drain, ΔP monitoring under 0.2 bar, modular cartridge design for rapid access and compact inline footprint.

Markets/applications section  : water treatment / seperation/ Compressed Air Systems

Related Products:  Oil Seperator/HVAC Filter/Air Filter
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Flow rate (m*/min) FIG D (mm) d (mm) H (mm) h1 (mm)
ws-150 3 (359 042 150 19
ws-250 3 59 342 250 19
ws-250 3 371 058 250 20
ws-350 3 @71 385 350 20
ws-375 282 375
ws-340 4 3120 080 340
ws-110 5 @42 110 20
ws-365 5 (362 365 100
ws-515 D 262 515 110
ws-630 5 084 630 70
ws-150 5 042 150 30
ws-165 5 262 165 50
ws-385 5 362 385 55
ws-320 5 284 520 95
ws-670 5 (084 670 95
ws-93 5 @42 93 25
ws-155 5 342 155 25
ws-310 5 062 310 50
ws-520 5 284 520 95
ws-670 5 084 670 95





