Wire Mesh Mist Eliminator
[image: Wire Mesh Mist Eliminator - Wire Mesh Demister]Arabo manufactures high‑performance knitted wire mesh mist eliminators alongside our pall rings, providing a fully integrated, customized separation package tailored to your process needs.
Our knitted mesh demister pads are precision‑engineered in stainless steel 304 and 316, delivering exceptional separation of droplets down to 2–5 µm. The multi‑layer, high‑void (> 95 %) mesh structure maximizes impaction and coalescence while maintaining low pressure drop (< 2 mbar). Ideal for gas‑liquid streams up to 300 °C, our pads are available in thicknesses from 100 mm to 300 mm, in diameters up to 6 m, with custom sectional assemblies for ease of installation.
· Material options: SS 304 or SS 316, corrosion‑resistant for harsh chemical and high‑temperature service
· Pad density: 145–190 kg/m³, free volume ≥ 95 %
· Droplet removal: effective for particles as small as 2 µm with > 99 % efficiency
· Typical pressure drop: under 2.5 mbar at design flow rates
· Modular design: sectional pads with rigid support grids for ease of handling and man‑way access
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